Status display-HD Encoder

HD Encoder System Platform
Version:

Language（语言）

# Status Display

## Input status

###

Running Time:

Device Time:(Sync Time To Device)

CPU Usage:

HDMI Input Size:

HDMI Video Frames:

HDMI Lost Video Frames:

CVBS Input Size:
CVBS Video Frames:
CVBS Lost Video Frames:

Audio Samplerate:

## WIFI

###

WIFI:Disable

###

WIFI:

SSID:

IP:

## Main stream

###

Encode Type:

Encoding Size:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL:

Multicast URL:

Preview(HTML5)

## Substream

###

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###

Encode Type:

Encoding Size:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL:

Multicast URL:

Preview(HTML5)

## CVBS1

###

Encode Type:

Encoding Size:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL:

Multicast URL:

Preview(HTML5)

## CVBS2

###

Encode Type:

Encoding Size:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL:

Multicast URL:

Preview(HTML5)